Water Level Detector PoC

Aliaxis

Authors:

Yunbo Hu

Damian Lee

Hawon Ryu

Aldonza Watt

Team 16

Date: 23 April

Abstract

This project, commissioned by Aliaxis, involves an analogue system designed to detect water level in a water tank. The system consists of a vertical probe, a transmitter and a receiver. The transmitter transmits a signal to the receiver using red light. The report

Table of contents

1. Introduction
   1. Client requirements
   2. Design tools and methodology
2. Water Level Probe
   1. Operation principles
   2. Optimised configuration
   3. Accuracy
3. Transmitter and Receiver
   1. Design of transmitter
   2. Minimization of signal loss
   3. Maximization of range
   4. Design of receiver
   5. Signal capture arrangement
4. Recommendations
   1. Battery
   2. Solar charging system
   3. Other recommendations
5. Conclusions

References

Bibliography

Appendix A – Bill of materials

Appendix B – Solar energy calculations

Introduction

Client requirements

Our client, Aliaxis, has asked for a few requirements for the design of the project. This involves accuracy, compliance, system stability, transmission (Tx) range and battery life.

Accuracy – An analysis should be conducted to determine the accuracy needed by the system sensor converting water level values into electronic measurements

Compliance – The device must transmit data without radio frequency (RF) emissions to avoid the system needing to meet and be tested

Design tools and methodology

In this project, our team used software for designing and simulating. FEMM was used to simulate the dielectric material of the water level probe, we compared the accuracy of the probe using 2 different materials. In addition of using software for design tools, we used LTSpice to simulate the circuit for the transmitter and receiver of the project, with

1. Water Level Probe
   1. Operation principles
   2. Optimised configuration  
      We were given 2 options for the dielectric material of the probe, silicone rubber and polyvinyl chloride (PVC).
   3. Accuracy